|  | Daily Tests | Weekly Tests | Chemicals Added, Maintenance & Notes |
| --- | --- | --- | --- |
| **Date** | **Water Clarity** | **Disinfectant: Free Chlorine Residual**Non-stabilized: 3.0 to 10.0 PPMStabilized: 3.5 to 10.0 PPM  | **Combined Chlorine**< 50% of free chlorine | **pH** 7.2-8.0 | **Temp**Max 104° F | **Flow Rate**GPM | **Alkalinity** Rec. Range60-160 PPM | **Cyanuric Acid** if used < 90 | Quantity of Disinfectant or Other Chem. added | Vacuum (V), Brush (B), or Back wash (BW) | Other Notes |
| 1 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 2 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 3 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 4 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 5 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 6 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 7 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 8 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 9 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 10 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 11 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 12 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 13 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 14 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 15 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |

** Spa, Wading, or Recirculating Spray Pool Log Sheet**

|  |
| --- |
| Pool Name Month Year Size of Pool (gallons) Flow Rate Required (GPM)  |
| Type of Disinfectant Minimum of 3.0 PPM if inorganic chlorine, 3.5 PPM if stabilized or organic, and 4.0 PPM if Bromine. |

|  | Daily Tests | Weekly Tests | Chemicals Added, Maintenance & Notes |
| --- | --- | --- | --- |
| **Date** | **Water Clarity** | **Disinfectant: Free Chlorine Residual**Non-stabilized: 3.0 to 10.0 PPMStabilized: 3.5 to 10.0 PPM  | **Combined Chlorine**< 50% of free chlorine | **pH** 7.2-8.0 | **Temp**Max 104° F | **Flow Rate**GPM | **Alkalinity** Rec. Range60-160 PPM | **Cyanuric Acid** if used < 90 | Quantity of Disinfectant or Other Chem. added | Vacuum (V), Brush (B), or Back wash (BW) | Other Notes |
| 16 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 17 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 18 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 19 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 20 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 21 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 22 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 23 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 24 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 25 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 16 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 27 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 28 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 29 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 30 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |
| 31 |       |       |       |       |       |       |       |       |       |       |       |       |       |       |       |

** Spa, Wading, or Recirculating Spray Pool Log Sheet (pg 2)**

|  |
| --- |
| Pool Name Month Year  |