|  | Daily Tests | | | | | | | | | | Weekly Tests | | Chemicals Added, Maintenance & Notes | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Water Clarity** | **Disinfectant: Free Chlorine Residual**  Non-stabilized:  3.0 to 10.0 PPM  Stabilized: 3.5 to 10.0 PPM | | | **Combined Chlorine** < 50% of free chlorine | | **pH**  7.2-8.0 | | **Temp**Max  104° F | **Flow Rate**  GPM | **Alkalinity** Rec. Range 60-160 PPM | **Cyanuric Acid**  if used < 90 | Quantity of Disinfectant or  Other Chem. added | Vacuum (V), Brush (B), or Back wash (BW) | Other Notes |
| 1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 4 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 5 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 6 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 7 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 8 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 9 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 10 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 11 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 12 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 13 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 14 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 15 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

** Spa, Wading, or Recirculating Spray Pool Log Sheet**

|  |
| --- |
| Pool Name Month Year Size of Pool (gallons) Flow Rate Required (GPM) |
| Type of Disinfectant Minimum of 3.0 PPM if inorganic chlorine, 3.5 PPM if stabilized or organic, and 4.0 PPM if Bromine. |

|  | Daily Tests | | | | | | | | | | Weekly Tests | | Chemicals Added, Maintenance & Notes | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Water Clarity** | **Disinfectant: Free Chlorine Residual**  Non-stabilized:  3.0 to 10.0 PPM  Stabilized: 3.5 to 10.0 PPM | | | **Combined Chlorine** < 50% of free chlorine | | **pH**  7.2-8.0 | | **Temp**  Max 104° F | **Flow Rate**  GPM | **Alkalinity** Rec. Range 60-160 PPM | **Cyanuric Acid**  if used < 90 | Quantity of Disinfectant or  Other Chem. added | Vacuum (V), Brush (B), or Back wash (BW) | Other Notes |
| 16 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 17 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 18 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 19 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 20 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 21 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 22 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 23 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 24 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 25 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 16 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 27 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 28 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 29 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 31 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

** Spa, Wading, or Recirculating Spray Pool Log Sheet (pg 2)**

|  |
| --- |
| Pool Name Month Year |